***Hardware and software requirements – FXT Feed Adapters***

**Supported operating system**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Windowns 7 service Pack 1 | Windowns 8 Update 1 | Windowns Server 2008 R2-SP1 | Windowns 10 | Windowns server 2012 & 2012 R2 | Windows server 16 |
| Enterprise  Professional  64-bit | Pro  Enterprise  64-bit | Standard  Enterprise  64-bit | Pro  Enterprise  64-bit | Standard  64-bit | Standard  64-bit |

*Không support bản 32-bit.*

**Cluster installion**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operating system** | **ISCSI** | **Memory server platform** | **CPU** |
| Windowns 2012 R2 – 64bit | 60GB | 4GB per server platform |  |

* **Khuyến nghị chọn giao diện FIX cho giải pháp STP (dịch vụ được cung cấp bởi Refinitiv) -> không phụ thuộc vào môi trường của khách hàng.**

**Refinitiv không đảm bảo hiệu suất của ứng dụng trên môi trường ảo hóa.**

* **Khuyến kích chạy trên môi trường vật lý vì xử lý lỗi trên môi trường ảo hóa sẽ phức tập hơn.**

**BROWSER:** Internet explorer 10 hoặc version cao hơn.

**Software:** Microsoft .Net framework 4.0 trở lên.